Riverside Drive – Phase II

CJA was contracted with Flatiron West, Inc. to install the CIDH piles for a two phase bridge that spans the Los Angeles River, the Metrolink rails, and is tucked between Interstate 5 & 110 Freeway. CJA is currently in the process of finishing the second phase of work, which includes 1 ea. 96-inch diameter and 22 ea. 24-inch wet CIDH Piles. The 96-inch diameter CIDH pile was completed while working between the Phase 1 Bridge and the Interstate 5 Highway. The tight access provided multiple challenges, from fitting the counter weights of the BG40 underneath the Phase 1 Bridge, to utilizing a 350 ton hydraulic crane with the assistance of a 75 ton crane to pick an 80,000 pound cage off the top of the Phase 1 Bridge. Multiple key personnel successfully managed and lent support for the critical CIDH work.

Click here to learn more about the Riverside Drive project.